## PPJoyCom virtual joystick

### Notes

- The PPJoyCom application reads data from the serial port and maps it to a virtual joystick. At the moment the only protocol supported is the FMSLead R/C interface. You need to load one instance of the mini-driver for each virtual joystick.
- You can specify a .ini file on the commandline to load a specific configuration on startup.
- You also need to configure a corresponding virtual joystick in PPJoy.

PPJoyCom can be found in the PPJoy installation directory
Back to PPJoy interface diagrams.