## Linux NES PowerPad interface

Controller | Parallel Port
--- | ---
Pad 1 | Pad 2
Power | +5v
Clock | 2
Latch | 3
Data 1 | 10 | 12
Data 2 | 11 | 13
Ground | 18

### Notes

- The PowerPad interface was developed by Juan Pablo Sousa. The PPJoy scanning code is also based on his original code for Linux.
- This interface supports an additional pad on pins 12 and 13.
- General notes about interface construction

### Credits

The original diagram and information for this interface can be found at http://insomnia.sourceforge.net/powerpad/.
Back to PPJoy interface diagrams.