## FMS PPM radio control

### Notes

- See the FMS manual for the various Parallel Port interfaces. PPJoy needs the PPM signal on pin 10 (IRQ).
- This interface still needs some work but should be usable. Particularly the timing is currently fixed at 1ms minimum pulse and 3ms max pulse. This means that you will have to calibrate your controller in the Game Controller control panel applet. Mapping buttons will (probably) also not work at this stage.
- This interface is only supported on Windows 2000/XP.
- General notes about interface construction.

### Credits

Diagrams and information for this interface can be found at http://www.csd.net/~cgadd/fms/fms_instruct2.htm#AnschlusseinerFernsteuerungandenParallelport, http://myweb.absa.co.za/eric.brouwer/interface.htm or http://www.heliguy.com/nexus/fmsinterface.html.
Back to PPJoy interface diagrams.